
Current local date and time: Tue Feb 17 2009 03:57:15

C++ version of Program B6-3
Newton - Raphson Solution then Levy Matching found in text:
Circuit Design Using Personal Computers
Thomas R. Cuthbert, Jr.
1983 John Wiley and Sons

Cuthbert_B6_3n .cpp .exe
Rev: n January 30, 2009
Steven Schultz, WB8WGY

Inputs:
   Text Result File Name:                Hubler_T1_N1_Series_Load.txt
   CSV Result File Name:                 Hubler_T1_N1_Series_Load.csv
   N =                                   1
   Low Frequency (f1) (MHz) =            25.000000
   High Frequency (f2) (MHz) =           30.000000
   Load Decrement obtained from Load Parameters
      Series Load Parameters entered
         average resistance (ohms) =     1.000000e+001
         delta bandwidth (MHz) =         1.000000e+000
         delta reactance (ohms) =        7.996750e+000

Output Part 1: Preliminary
   Center Frequency     (f0)    (MHz) =      27.386128
   Match Bandwidth      (f2-f1) (MHz) =      5.000000
   Fractional Match Bandwidth ((f2-f1)/f0) (wm) =  0.182574186
   Reactance Slope Parameter =               1.095000090e+002
   Load Decrement =                          5.002032076e-001
   Load Q =                                  1.095000090e+001

Output Part 2: Fano; Levy; Newton - Raphson Solution
   FV =                   5.201e-010
   IT (iterations in Newton - Raphson Solution) = 12
   A  =                   1.258684039
   B  =                   0.584175177
   Magnitude of Reflection Coefficient Min = 0.381846776
   Magnitude of Reflection Coefficient Max = 0.617921762
   Mismatch Loss Min (dB) = -0.684439717
   Mismatch Loss Max (dB) = -2.088901811
   Return Loss Min (dB) = -8.362217440
   Return Loss Max (dB) = -4.181330191
   SWR Min =              2.235443773
   SWR Max =              4.234530002

Output Part 3: Resistive Source with g(i) Prototype Values
   G(0) (load)   =     1.000000000
   G(1)          =     1.999187500
   G(2) (source) =     0.447338614

Output Part 4: Network Element Values Calculated
   Load Resistance (ohms) =   1.000000000e+001
   L(1) (H) =                 6.363611456e-007
   C(1) (F) =                 5.307320869e-011
   Source Resistance (ohms) = 2.235443058e+001
