
Current local date and time: Tue Feb 17 2009 04:02:19

C++ version of Program B6-3
Newton - Raphson Solution then Levy Matching found in text:
Circuit Design Using Personal Computers
Thomas R. Cuthbert, Jr.
1983 John Wiley and Sons

Cuthbert_B6_3n .cpp .exe
Rev: n January 30, 2009
Steven Schultz, WB8WGY

Inputs:
   Text Result File Name:                Hubler_T1_N2_Series_Load.txt
   CSV Result File Name:                 Hubler_T1_N2_Series_Load.csv
   N =                                   2
   Low Frequency (f1) (MHz) =            25.000000
   High Frequency (f2) (MHz) =           30.000000
   Load Decrement obtained from Load Parameters
      Series Load Parameters entered
         average resistance (ohms) =     1.000000e+001
         delta bandwidth (MHz) =         1.000000e+000
         delta reactance (ohms) =        7.996750e+000

Output Part 1: Preliminary
   Center Frequency     (f0)    (MHz) =      27.386128
   Match Bandwidth      (f2-f1) (MHz) =      5.000000
   Fractional Match Bandwidth ((f2-f1)/f0) (wm) =  0.182574186
   Reactance Slope Parameter =               1.095000090e+002
   Load Decrement =                          5.002032076e-001
   Load Q =                                  1.095000090e+001

Output Part 2: Fano; Levy; Newton - Raphson Solution
   FV =                   2.513e-010
   IT (iterations in Newton - Raphson Solution) = 13
   A  =                   0.979852631
   B  =                   0.424124097
   Magnitude of Reflection Coefficient Min = 0.274194313
   Magnitude of Reflection Coefficient Max = 0.381827116
   Mismatch Loss Min (dB) = -0.339439708
   Mismatch Loss Max (dB) = -0.684363383
   Return Loss Min (dB) = -11.238831146
   Return Loss Max (dB) = -8.362664656
   SWR Min =              1.755558458
   SWR Max =              2.235340876

Output Part 3: Resistive Source with g(i) Prototype Values
   G(0) (load)   =     1.000000000
   G(1)          =     1.999187500
   G(2)          =     0.400088508
   G(3) (source) =     2.235341388

Output Part 4: Network Element Values Calculated
   Load Resistance (ohms) =   1.000000000e+001
   L(1) (H) =                 6.363611456e-007
   C(1) (F) =                 5.307320869e-011
   L(2) (H) =                 2.651995580e-008
   C(2) (F) =                 1.273521273e-009
   Source Resistance (ohms) = 2.235341388e+001
