
Current local date and time: Tue Feb 17 2009 04:16:18

C++ version of Program B6-3
Newton - Raphson Solution then Levy Matching found in text:
Circuit Design Using Personal Computers
Thomas R. Cuthbert, Jr.
1983 John Wiley and Sons

Cuthbert_B6_3n .cpp .exe
Rev: n January 30, 2009
Steven Schultz, WB8WGY

Inputs:
   Text Result File Name:                Hubler_T1_N2_Parallel_Load.txt
   CSV Result File Name:                 Hubler_T1_N2_Parallel_Load.csv
   N =                                   2
   Low Frequency (f1) (MHz) =            25.000000
   High Frequency (f2) (MHz) =           30.000000
   Load Decrement obtained from Load Parameters
      Parallel Load Parameters entered
         average conductance (Siemens) = 8.263954e-004
         delta bandwidth (MHz) =         1.720000e-001
         delta susceptance (Siemens) =   1.137166e-004

Output Part 1: Preliminary
   Center Frequency     (f0)    (MHz) =      27.386128
   Match Bandwidth      (f2-f1) (MHz) =      5.000000
   Fractional Match Bandwidth ((f2-f1)/f0) (wm) =  0.182574186
   Susceptance Slope Parameter =             9.053073689e-003
   Load Decrement =                          4.999798052e-001
   Load Q =                                  1.095489361e+001

Output Part 2: Fano; Levy; Newton - Raphson Solution
   FV =                   2.510e-010
   IT (iterations in Newton - Raphson Solution) = 13
   A  =                   0.979702179
   B  =                   0.424204099
   Magnitude of Reflection Coefficient Min = 0.274343768
   Magnitude of Reflection Coefficient Max = 0.381979732
   Mismatch Loss Min (dB) = -0.339824712
   Mismatch Loss Max (dB) = -0.684956083
   Return Loss Min (dB) = -11.234098014
   Return Loss Max (dB) = -8.359193602
   SWR Min =              1.756125989
   SWR Max =              2.236139823

Output Part 3: Resistive Source with g(i) Prototype Values
   G(0) (load)   =     1.000000000
   G(1)          =     2.000080782
   G(2)          =     0.399981308
   G(3) (source) =     2.236140335

Output Part 4: Network Element Values Calculated
   Load Resistance (ohms) =   1.210074499e+003
   L(1) (H) =                 6.419385317e-007
   C(1) (F) =                 5.261209012e-011
   L(2) (H) =                 1.540642707e-005
   C(2) (F) =                 2.192184322e-012
   Source Resistance (ohms) = 5.411442568e+002
